If the firmware update fails on your RD-5R, please find the **vcredist\_x86\_2008** file in the **Firmware software V3.1.6--update software** document and run it first. It is a database that can help you solve the error.



After the database is iupdated, please restart your computer and follow the instruction below:

1. Turn off the radio and then plug in the programming cable.
2. Hard press the side key 1 and the side key 2 for one second and then turn on the radio (still pressing the keys). The radio will be in upgrade mode when the indicator light is on.



3.Open the upgrade software "Update.exe"



4. Click "Browse" to select the file to be upgraded, for example: RD-5R\_V2.1.0.sgl,



5. Click "Download" to complete the upgrade.





6. Unplug programming cable, turn off radio or reboot