**UV 008 upgrade operation method**


1. Upgrade software version number：C7000 IAP Tool V2.15
2. Operating instructions：
3. Install the UV008 handset battery, plug in the ordinary Jianwu write frequency cable and connect the computer USB port。



1. Press and hold the three side keys on the handset to start up, and the traffic lights will light up together.



1. Open upgrade folder (UV008 firmware upgrade).
2. Double-click“IAP Tool.exe”微信图片_20211202155557
3. Operation interface

****

1. After selecting all options, click to start the upgrade.。
2. Just reboot after the upgrade。